{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Abmessungen","Maßeinheit","","Höhe","mm","870","870"]
["","","","Breite","mm","1,100","1,100"]
["","","","Tiefe","mm","460","460"]
["Gewicht","Maßeinheit","","","kg","117","117"]
["Verdichter","Type","","","","Hermetischer Scrollverdichter","Hermetischer Scrollverdichter"]
["Betriebsbereich","Kühlen","Umgebung","Min.","°C Trockenkugel","-20","-20"]
["","","","Max.","°C Trockenkugel","46","46"]
["","Heizen","Umgebung","Min.","°C Feuchtkugel","-20","-20"]
["","","","Max.","°C Feuchtkugel","15","15"]
["Schallleistungspegel","Kühlen","","","dBA","73","76"]
["","Heizen","","","dBA","76 (1)","79 (1)"]
["Schalldruckpegel","Kühlen","","Nom.","dBA","53","57"]
["","Heizen","","Nom.","dBA","60","63"]
["Kältemittel","Typ","","","","R-32","R-32"]
["","Charge","","","kg","5","5"]
["","GWP","","","","675","675"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","9.52","9.52"]
["","Gas","","AD","mm","22.2","22.2"]
["","Leitungslänge","Max.","Außengerät – Innengerät","m","100","100"]
["","","System","Unbefüllt","m","30","30"]
["","Zusätzliche Kältemittelfüllmenge","","","kg/m","Siehe Installationsanleitung","Siehe Installationsanleitung"]
["Standardzubehör","Installationsanleitung","","","","1","1"]
["","Allgemeine Schutzmaßnahmen","","","","1","1"]
["","Kabelbinder","","","","2","2"]
["","F-Gase-Aufkleber abziehen","","","","1","1"]
["","Verbindungsleitungen","","","","6","6"]
["Power supply","Phase","","","","3~","3~"]
["","Frequenz","","","Hz","50","50"]
["","Spannung","","","V","380-415","380-415"]
["Strom - 50 Hz","Max. Amperezahl für Sicherung (MFA)","","","A","20","20"]
["Hinweise","","","","","(1) - Gemäß ENER Lot 21","(1) - Gemäß ENER Lot 21"]